**SCRAP ACCEPTANCE POLICY**

To maintain an environmentally friendly, safe and efficient operation here at Recon Metal, there are certain materials we cannot accept.

Please be sure that your scrap loads do NOT contain any of the following materials:

1. Alkaline, Lithium ion, and Cadmium bearing (ie. nickel cadmium) batteries.
2. Asbestos and any asbestos containing materials (ie. pipe or I-beam insulation and other structural demolition debris).
3. Automobiles with air bags containing sodium azide.
4. Barbed wire, chain link fencing or chicken wire.
5. Batteries that are cracked, broken, burned or have missing caps.
6. Brake chambers/brake pots unless the spring is cut.
7. Brake shoes.
8. Cans that contained paint, water sealer, pesticides or other toxic chemicals.
9. Cathode ray tubes (CRTs) and liquid crystal displays (LCDs), or any commodity containing a CRT or LCD, such as computer monitors, laptop screens, and televisions.
10. Closed containers and compressed cylinders and tanks unless punctured and valve is removed.
11. Combustible or explosive materials.
12. Composite Aluminum.
13. Concrete Bollards.
14. Fiber optic cable.
15. Fluorescent, neon, or mercury vapor lights and related fixtures.
16. Free flowing fluids of any kind including water.
17. Gasoline, diesel, propane or other petroleum product containers unless they are open, punctured, fully drained and the inside is fully visible.
18. Landfill material such as dirt, debris, trash or waste of any kind (ie. tires, wood, dirt, yard debris, concrete, asphalt, glass, rubber or other non-metallic materials).
19. Materials such as capacitators, ballasts and transformers containing Polychlorinated biphenyls (PCB’s).
20. Microwaves unless the capacitor is removed.
21. Oil cans, oil filters and undrained oil pans still on motor blocks. This includes hydraulic fluids, gear oils and grease. Hydraulic equipment must have hydraulic hoses removed and cylinders cut open and drained.
22. Paint cans or aerosol containers unless opened, empty and cleaned.
23. Plastic dishwashers.
24. Radioactive material of any kind.
25. Safes containing concrete.
26. Slag.
27. Steel cable or wire rope unless cut to lengths of 4 feet or shorter.
28. Tar or materials with residual tar (ie. tar kettle).
29. Tires with steel rims.
30. Wet drums of any size unless empty, dry and odor free with the top removed.
31. Wooden trailers, recreational vehicles and cube vans.

APPROVAL REQUIRED PRIOR TO THE SALE OF THE FOLLOWING MATERIALS:

1. Any non-lead acid batteries.
2. ATMs (documentation required).
3. Bandings.
4. Kegs.
5. Light fixtures containing ballasts.
6. Loose honeycomb from catalytic converters or dpfs.
7. Manhole covers and catch basins (documentation required).
8. Medical equipment or instruments (must be sterilized and free of biohazardous waste).
9. Munitions scrap (exception: range lead and brass shells ok).
10. Precious metals.
11. Railroad scrap (documentation required).
12. Shopping carts.
13. Skulls.
14. Steel turnings.

FEES:

* Brake chambers - **$5/unit**
* Accumulators and pressurized cylinders - **$50/unit**
* Any undrained tank on farm equipment and large forklifts- **$50/unit**
* Undrained refrigeration and AC units - **$15/unit**
* Landfill Material – (garbage, concrete, plastic, etc) - **$0.07/lb**
* Undrained propane tanks on vehicles - **$50/unit**